

***Device Under Test***

|  |  |
| --- | --- |
| ***Asset Number:*** <AssetNumber> | ***Serial Number:*** <SerialNumber> |
| ***Location:*** <Location>  ***Manufacturer:*** <Manufacturer> | ***Model:*** <Model> |

***Test Equipment:***

<Items>

***Signatures***

|  |  |
| --- | --- |
| Name: <Name> | Date: <Date> |

***Performance Test Results***

***Performance Verification:***

|  |  |
| --- | --- |
| Visual Inspection for no damage | **<result1>** |
| Set Defibrillator Analyser to Vfib and AED leads connected, ensure  AED charges up to Automatic Energy Selection (Specify: 200 Joules)  and delivers shock ± 10% | **<result2>** |
| Set the Defibrillator Analyser to normal QRS rhythm.  Ensure AED monitors and displays the waveform, no shock  advised | **<result3>** |
| Overall performance | **<result4>** |

***Parts and Comments:***

<Comments>