|  |  |  |
| --- | --- | --- |
| ***Equipment Description****:*  Twin-O-Vac Suction Device | | |
| ***Asset Number****:* <AssetNumber> | ***Serial Number:*** <SerialNumber> | |
| ***Make****:* <Make> | ***Model:*** <Model> | |
| Visual Inspection | | **<result1>** |
| Suction /L - 60kpa, No Leak | | **<result2>** |
| Flow O2 Outlets 120 lpm | | **<result3>** |
| No Leaks | | **<result4>** |
| Bacteria Filter | | **<result5>** |
| Overall Test Result | | **<result6>** |
| *Comments:*  <Comments> | | |
| *Parts:* | | |