

***Queensland Ambulance Service Report***

|  |  |
| --- | --- |
| ***Date:*** 5/04/2017 | ***Station:*** dasdas |
| ***Location/Room:*** dasd  ***Registration Number:*** asd | ***Vehicle Number:*** asdsa |

***Test Summary***

|  |  |
| --- | --- |
| ***List of Serviced Equipment:***   * Outlet Point: 1 * Oxygen Reticulation: 1 * Sphygmo Wall: 1 | ***List of Parts Replaced:***   * a * c * dasd |

***Signatures***



|  |  |
| --- | --- |
| Name: Rommel Lapuz | Date: 5/04/2017 |

***Test Results***

|  |  |  |
| --- | --- | --- |
| ***Equipment Description****:*  Outlet Point | | |
| ***Asset Number****:* a | ***Serial Number:*** dasd | |
| ***Make****:* sda | ***Model:*** sd | |
| Leak Test at Pipeline Pressure 400 KpA | | **Pass** |
| Visual Inspection | | **Pass** |
| Pressure Drop Test with Cyclinders Off | | **Pass** |
| Overall Test Result | | **Pass** |
| *Comments:* | | |
| *Parts:*  c | | |

|  |  |  |
| --- | --- | --- |
| ***Equipment Description****:*  Oxygen Reticulation Failure Alarm | | |
| ***Asset Number****:* asdd | ***Serial Number:*** sadasd | |
| ***Make****:* dasdasd | ***Model:*** d | |
| No Supply Left Ensure Alarm | | **Pass** |
| Alarm | | **Pass** |
| Alarm Clears | | **Pass** |
| Overall Test Result | | **Pass** |
| *Comments:* | | |
| *Parts:*  a | | |

|  |  |  |
| --- | --- | --- |
| ***Equipment Description****:*  Sphygmo Wall | | |
| ***Asset Number****:* asdasd | ***Serial Number:*** sada | |
| ***Make****:* asdas | ***Model:*** dsa | |
| Check Needle in Calibration Zone @ Zero mmHg | | **Pass** |
| Check Pressue @ 0mm Hg +/- 10% | | **Pass** |
| Check Pressue @ 100mm Hg +/- 10% | | **Pass** |
| Check Pressue @ 200mm Hg +/- 10% | | **Pass** |
| Check No Leaks | | **Pass** |
| Overall Test Result | | **Pass** |
| *Comments:* | | |
| *Parts:*  dasd | | |