|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | |  | | --- | | **Test - All** | | |  | | --- | | bl | |  | | |  | | --- | |  | |  | |  |  | |  |  |  | | | | | |  |
| |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | | **Model** | **Serial Number** | **Test Name** | **Date** | **Status** | **Result** | **Technician** | | 8110 Syringe | <serialnumber> | Instrument Inspection | <date> | Complete | Pass | Nova Biomedical | | 8110 Syringe | <serialnumber> | Binary Switches | <date> | Complete | Pass | Nova Biomedical | | 8110 Syringe | <serialnumber> | Pressure Disc Accuracy | <date> | Complete | Pass | Nova Biomedical | | 8110 Syringe | <serialnumber> | Barrel Clamp Accuracy | <date> | Complete | Pass | Nova Biomedical | | 8110 Syringe | <serialnumber> | Plunger Force Accuracy | <date> | Complete | Pass | Nova Biomedical | | 8110 Syringe | <serialnumber> | Plunger Position Accuracy | <date> | Complete | Pass | Nova Biomedical | | 8110 Syringe | <serialnumber> | Simultaneous Display | <date> | Complete | Pass | Nova Biomedical | | 8110 Syringe | <serialnumber> | IUI Connectors | <date> | Complete | Pass | Nova Biomedical | | 8110 Syringe | <serialnumber> | Alarm | <date> | Complete | Pass | Nova Biomedical | | 8110 Syringe | <serialnumber> | Keypad | <date> | Complete | Pass | Nova Biomedical | | 8110 Syringe | <serialnumber> | Analog Sensors | <date> | Complete | Complete | Nova Biomedical | | | | |  |  |
|  |  |  |  |  |  |
|  | |  | | --- | | Signature | | |  |  |  |