|  |  |
| --- | --- |
| ***Equipment Description:***  Twin-O-Vac Suction Device | |
| ***Asset Number:*** <AssetNumber> | ***Serial Number:*** <SerialNumber> |
| ***Make:*** <Make> | ***Model:*** <Model> |

|  |  |
| --- | --- |
| Visual Inspection | **<result1>** |
| Suction /L - 60kpa, No Leak | **<result2>** |
| Flow O2 Outlets 120 lpm | **<result3>** |
| No Leaks | **<result4>** |
| Bacteria Filter | **<result5>** |
| Overall Test Result | **<result6>** |

***Comments/Parts:***

<Comments>

***--------------------------------------------------------------------------------------------------------------------------***